# TerminalInfo ActiveX control

The TerminalInfo ActiveX control allows an HMI application to read the following PanelView Plus 7 and PanelView Plus 6 hardware attributes and write the values to tags:

- CPU Temperature
- Logic Board Temperature
- Display Temperature
- Battery Voltage
- CPU Load
- Memory Load
- Memory (BinFS) Thrashing
- Device Name
- Internal NIC IP Address
- Internal NIC Subnet Address
- Internal NIC Gateway Address
- Internal NIC MacID
- External NIC IP Address
- External NIC Subnet Address
- External NIC Gateway Address
- External NIC MacID

## See also

Connections for the TerminalInfo ActiveX control