# Options on the Timing tab of the Piloted Control List Selector Properties dialog box

The following table shows the options on the Timing tab of the Piloted Control List Selector Properties dialog box.

Options | Descriptions
--- | ---
Timing and handshaking settings |
Enter key control delay | Select the time to delay between the time the operator presses the Enter button and the time the application sets the Enter connection to 1.
Enter key hold time | Select the time the Enter connection will be set to 1. This time setting applies only if the Enter connection is assigned and the Enter Handshake connection is not assigned.
Enter key handshake time | Select the maximum time the Enter connection will be set to 1. This time setting applies only if the Enter and Enter Handshake connections are both assigned.
Handshake reset type | Select how the Enter Handshake connection resets the Enter connection to 0: Non-zero value resets the Enter connection when the Enter Handshake connection is a non-zero value. Zero to non-zero transition resets the Enter connection when the Enter Handshake connection changes from 0 to a non-zero value.

## See also

Create piloted control list selectors

Configure the piloted control list selector

Set up states for the piloted control list selector

Set up connections for the piloted control list selector

How the piloted control list selector works at run time