# InactiveAcknowledged connection

The InactiveAcknowledged connection specifies whether to display alarms that are currently inactive (no longer in alarm) and have also been acknowledged.

A read-only connection. You can assign a tag or an expression to this connection. If you assign an expression, the application calculates the value of the expression and uses the result to determine whether or not to display inactive acknowledged alarms.

If this connection is assigned, it overrides the displayInactiveAckedAlarms attribute.

The alarmList graphic object element contains this connection.

## See also

connections and connection elements