# Close Display connection

A write connection. Assign a digital tag to this connection to notify the data source that the pop-up alarm display has been closed.

When the application starts, this connection has a value of zero. If the pop-up alarm display specified in the Alarm Setup editor closes, the connection is set and held for the duration of the notification hold time, and is then reset to 0.