# IPInfo ActiveX control

The IPInfo ActiveX control provides the system with the ability to read the hosting PanelView Plus terminal's TCPIP settings.

Use the IPInfo ActiveX control to read:

- Terminal IP address as a stringRead
- Individual terminal IP address octets as separate values
- Terminal subnet mask address as a string
- Individual terminal subnet mask address octets as separate values
- Terminal gateway address as a string
- Individual terminal gateway address octets as separate values
- Terminal MAC ID as a string

## See also

Connections for the IPInfo ActiveX control