# Controller instruction faceplates tag passing

The following table indicates the contents that are expected to be contained within parameter files passed to the faceplates for an instruction to provide full functionality.

Note that the arrays passed to the RMPS faceplates are expected to be of length 10 or less. You will be required to modify the RMPS and RMPS_Config faceplates to add additional segments.

Instruction Name | Displays | Placeholder Tags
Logix_ALM | Logix_ALM Logix_ALM_Status Logix_ALM_Config | #1= Backing tag
Logix_ALMA | Logix_ALMA Logix_ALMA_Status Logix_ALMA_Config | #1= Backing tag
Logix_ALMD | Logix_ALMD Logix_ALMD_Status Logix_ALMD_Config | #1= Backing tag
Logix_D2SD | Logix_D2SD Logix_D2SD_Status | #1= Backing tag
Logix_D3SD | Logix_D3SD Logix_D3SD_Status | #1= Backing tag
Logix_ESEL | Logix_ESEL Logix_ESEL_Status | #1= Backing tag
Logix_PhaseManager | Logix_PhaseManager | #1=Phase Tag
Logix_PIDE | Logix_PIDE Logix_PIDE_Status Logix_PIDE_Config Logix_PIDE_Trend Logix_PIDE_Tune Logix_PIDE_Autotune | #1= Backing tag #2=Autotune tag (if used)
Logix_RMPS* | Logix_RMPS Logix_RMPS_Status Logix_RMPS_Config | #1= Backing tag #2=Ramp Value Array #3=Soak Value Array #4=Soak Time Array
Logix_TOT | Logix_TOT Logix_TOT_Status Logix_TOT_Config | #1= Backing tag

## See also

About controller instruction faceplates

Controller instruction faceplates display list

Add a segment number "n" to Logix_RMPS Main Faceplate

Add a segment number "n" to Logix_RMPS_Config Faceplate

Backing Tag