# Value connection (pilotedControlListSelector)

When a display containing a piloted control list selector is opened, if the list is operator controlled, (that is, if the Remote Access connection's value is set to zero), the application reads this tag to determine what state to show.

A write connection. Assign a tag to this connection.

The pilotedControlListSelector graphic object element's connections element contains this connection.

## See also

connections and connection elements

Remote Access connection