# Status connection values

The following table shows the values returned by the Status connection.

Values | Descriptions
0x01 (Hex) or 1 (Dec) | Downloading
0x02 (Hex) or 2 (Dec) | Download succeeded
0x04 (Hex) or 4 (Dec) | Download with errors
0x11 (Hex) or 17 (Dec) | Uploading
0x12 (Hex) or 18 (Dec) | Upload succeeded
0x14 (Hex) or 20 (Dec) | Upload with errors
0x21(Hex) or 33 (Dec) | Deleting
0x22(Hex) or 34 (Dec) | Delete succeeded
0x24(Hex) or 36 (Dec) | Delete with errors

See also

Recipe 2 Enhanced ActiveX control

Connections for the Recipe 2 Enhanced ActiveX control