# InactiveUnacknowledged connection

The InactiveUnacknowledged connection specifies whether to display alarms that are currently inactive (no longer in alarm) and have not yet been acknowledged.

A read-only connection. You can assign a tag or an expression to this connection. If you assign an expression, the application calculates the value of the expression and uses the result to determine whether or not to show inactive unacknowledged alarms.

If this connection is assigned, it overrides the displayInactiveUnackedAlarms attribute.

The alarmList graphic object element contains this connection.

## See also

connections and connection elements