# Configure the MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal for remote audits

To collect audit messages from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal on the FactoryTalk computer, you need configure the terminal for remote audits.

## To configure the MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal for remote audits

1. On the terminal, start FactoryTalk View Machine Edition Station.
2. Select Terminal Settings > Diagnostics Setup > Remote Log and click Edit.
3. In the Address text box, enter the IP address of the FactoryTalk computer.
4. In the Port text box, enter the port number from the FactoryTalk computer and click OK.
5. In the Diagnostics Setup dialog box, select Message Routing and click Edit.
6. Select Remote Log and press Enter.
7. To ensure the capturing of all available information, select all the check boxes in the Remote Log Message Routing dialog box and click OK.

For the changes to take effect, restart the terminal.

## See also

Audit messages from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal

Configure the FactoryTalk computer for remote audits