# ErrorMessage connection values

The following table shows the ErrorMessage connection values.

Error codes | Error messages
0 | No error has occurred.
1 | Operation is successful.
2 | Operation has failed. Cannot get the interface to execute Macro.
3 | Index property is out of range. Range is 1 to 100.
4 | Macro_XX property has not been configured.
5 | The macro configured in Macro_XX property does not exist.

## See also

MacroMultiplexer ActiveX control

Connections for the MacroMultiplexer ActiveX control