# Set up handshaking for the piloted control list selector

When the operator presses the Enter key, the application writes a value to the data source. Use Enter key handshaking to hold the value at the data source for a specific period of time to ensure it is read before the operator sends a new value to the Value connection.

## To set up handshaking for the control list selector’s buttons

1. In the Graphics Display editor, double-click the object to open its Properties dialog box.
2. Click the Timing tab.
3. Specify the handshaking settings to use with the Enter key.

## See also

Create piloted control list selectors

Set up general properties for a piloted control list selector object

Set up states for a piloted control list selector

Options on the Timing tab of the Piloted Control List Selector Properties dialog box

Set up connections for the piloted control list selector