# Transfer a file from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal

Use the Upload tab of the Transfer Utility dialog box to transfer runtime application files (.mer) from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal to a development computer.

Before you transfer an application file, you must configure an FactoryTalk Linx driver for the transfer on the terminal and the computer.

To transfer a file from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal

1. On the Upload tab of the Transfer Utility dialog box, from the Select source terminal list, select the source terminal in the FactoryTalk Linx communications tree.
2. From the Source storage type list, select the kind of storage the file is stored in on the terminal.
3. In the Source file box, specify the file to be transferred. Click the Browse button to browse for the file.
4. (Optional) If you want to use a different name for the uploaded file, select Upload as and type the new name.
5. In the Destination folder box, specify the location on the destination computer to upload the file to. Click the Browse button to browse for the destination.

   Tip: | The destination must be on the local computer. ME Transfer Utility does not support uploading to a network location.

6. Click Upload.

The selected file starts to be uploaded to the destination folder.

## See also

About ME Transfer Utility

Configure download drivers

Options on the Upload tab

Keywords: transfer, upload