# InactiveAcknowledged

A read-only connection. Assign a tag or an expression to this connection. At run time, when the tag or expression value is non-zero, the Alarm list displays alarms that are no longer active but have been acknowledged.

If you assign an expression to this connection , the application calculates the value of the expression and uses the result to determine whether to show inactive acknowledged alarms.

When this connection is assigned, it overrides the DisplayInactiveAckedAlarms property.

## See also

DisplayInactiveAckedAlarms