# Connections for the Custom String Popup Keyboard ActiveX control

The following table shows the connections to control the operation of the Custom String Popup Keyboard ActiveX control at run time.

Connections | Descriptions
Value Required | The configured tag contains the user-entered string returned by the control. The connection is write-only and can be a memory or direct reference tag. The connection data type is String.
Launch Enable Required | When the configured tag transitions from zero (0) to non-zero, the keyboard will be shown to the user. The connection is read-only and can be a memory or direct reference tag. The connection data type is Analog.

## See also

Custom String Popup Keyboard ActiveX Control

Properties on the General tab of the ME Custom String Popup Keyboard Properties dialog box

Popup keyboard definition file

Keys with predetermined functions