# PanelView Plus 7 Standard applications and Compact Machine Edition applications

PanelView Plus 7 Standard applications and Compact Machine Edition applications (applications running on PanelView Plus 6 Compact or PanelView Plus Compact terminals) have the following restrictions:

Restrictions | PanelView Plus 7 Standard applications | Compact Machine Edition applications
Maximum number of displays | 100 (50 On Top displays and 50 Replace displays) | 25
Maximum number of alarm messages | 500 | 200
Maximum screen resolution | 1280x800 | 640x480
Maximum number of FactoryTalk Linx shortcut | 1 | 1
Methods of communications | Ethernet If the application uses FactoryTalk Linx, only Ethernet drivers are supported. | Serial and Ethernet If the application uses FactoryTalk Linx, only Serial-DF1, Serial-DH485, and Ethernet drivers are supported.
Supported versions of FactoryTalk Linx | 5.20 and later | 5.20 and later

If no FactoryTalk Linx shortcut is defined, a single KEPServer Enterprise data server can be used to communicate with a single device.

The Kepware Hilscher Universal and Modbus Plus communications drivers are not supported for PanelView Plus 7 Standard, PanelView Plus 6 Compact, or PanelView Plus Compact terminals. However, the drivers are supported on PanelView Plus 6 Compact 1000 terminal.

## See also

Create an application

Import and conversion of an application

Specify project settings (General tab)

Validate PanelView Plus 7 Standard applications and Compact Machine Edition applications

Open applications