# Remote Macro1-5

Assign these controls to allow the data source to control when Macros 1 through 5 are run.

At run time, when the tag value, or the result of the expression, assigned to Remote Macro1 (Remote Macro2, etc.) changes from a zero to a non-zero value, or from a non-zero value to a new non-zero value, the macro named Macro1 (Macro2, etc.) will be run.

## See also

Set up global connections - Macro tab