# Options on the Upload tab

The following table shows the options on the Upload tab.

Options | Descriptions
Source storage type | Options include: Internal Storage External Storage 1 External Storage 2
Source file | Type the path to the source file or click the Browse button (…) to open the Select File dialog box, browse for the source file, and click OK.
Upload as | If you want to rename the file that is transferred to the destination, select this check box, and in the box, type the new name. The name must not contain any of the following characters: \ / : * ? " < > . Do not specify a path. The name will automatically be given the same file extension as the file in the Source file box. If you type an extension, it must be the same as that of the source file. If you clear this check box, the file will be saved at the destination under the name that appears in the Source file box. This name will appear in the box, but will not be available for edit. If the file exists at the destination, you will be prompted to overwrite it.
Destination folder | Specify where on the destination computer you want to store the file.
Select source terminal | The FactoryTalk Linx communication tree shows all the hardware available on the network.

## See also

Transfer a file from a MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, or PanelView Plus CE terminal

Runtime application file folders on MobileView, PanelView Plus 7, PanelView Plus 6, PanelView Plus, PanelView Plus Compact, and PanelView Plus CE terminals