# Connections for the TerminalWakeUp ActiveX control

She following table shows the connections to control the operation of the TerminalWakeUp ActiveX control at run time.

Connections | Descriptions
Event Trigger Optional | When the assigned tag transitions from zero to non-zero, the control causes the PanelView Plus 7 or PanelView Plus 6 terminal to exit screen saver mode. The connection can be a tag, a tag placeholder (for example, "{#1}"), or expression. An application can use both triggers in the same control instance.
ChangeOfState Trigger Optional | When the assigned tag changes state from the last triggering value, the control causes the PanelView Plus 7 or PanelView Plus 6 terminal to exit screen saver mode. The connection can be a tag, a tag placeholder (for example, "{#1}"), or expression. The initial triggering value is zero. The triggering value is not persisted between application (MER) execution, nor power cycles. An application can use both triggers in the same control instance.

## See also

TerminalWakeUp ActiveX control

ChangeOfState Trigger connection example