# Causes of run-time errors for the multistate indicator

The error state is shown at run time if any of the following are true:

- The Indicator connection does not have a tag or an expression assigned to it
- The Trigger type is set to Value and the Indicator connection value does not match one of the configured state values
- The Trigger type is set to LSB and the position of the least significant bit set in the Indicator connection does not match one of the configured state values
- The Trigger type is set to Value and an array tag has been assigned to the object's Value connection

## See also

Create multistate indicators

Configure the multistate indicator (General tab)

Set up states for the multistate indicator (States tab)

How the multistate indicator works at run time

Example: Use a multistate indicator